|  |  |
| --- | --- |
| Transmitted by the expert from The International Automotive Lighting and Light Signalling Expert Group (GTB) | Informal document **GRE-72-11**(72nd GRE, 20 - 22 October 2014,agenda item 4 (d)) |

**Proposal for Supplement 24 to the 02 series of Regulation No.7 (Position, stop and end-outline lamps)**

**I.** **Proposal**

*Paragraph 1.6.,* amend to read:

“1.6. "*Front and rear position lamps, stop-lamps and end-outline marker lamps of different type"* meanslamps which differ in such essential respects as:

(a) The trade name or mark;

(b) The characteristics of the optical system (levels of intensity, light distribution angles, category of light source, light source module, etc.);

(c) ~~The system used to reduce illumination at night - in the case of stop-lamps with two levels of intensity.~~ **The variable intensity control, if any.**

A change of the colour of the light source or the colour of any filter does not constitute a change of type.”

 II. Justification

To correct an error introduced by Supplement 21 to the 02 series of Regulation No.7 by ECE/TRANS/WP29/2012/65 (ECE/TRANS/WP.29/GRE/2011/8)