|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRSP/2016/12 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  26 February 2016  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on Passive Safety**

**Fifty-ninth session**

Geneva, 9-13 May 2016

Item 9 of the provisional agenda

**Regulation No. 16 (Safety-belts)**

Proposal for Supplement 8 to the 06 series of amendments to Regulation No. 16 (Safety-belts)

Submitted by the expert from Denmark[[1]](#footnote-2)\*

The text reproduced below was prepared by the expert from Denmark to clarify the installation of safety-belts in vehicle category N3 in Annex 16 of the UN Regulation. The modifications to the current text of UN Regulation No. 16 are marked in bold for new or strikethrough for deleted characters.

I. Proposal

*Annex 16,*

*The table,* amend to read:

"Annex 16

3

ECE/TRANS/WP.29/GRSP/2016/12

Safety-belt installation showing the belt types and retractor types

| *Minimum requirements for safety-belts and Retractors* | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *Vehicle category* | *Forward facing seating positions* | | | | | | *Rearward-facing*  *seating positions* | *Side-facing seating position* |
| *Outboard seating positions* | | *Centre seating position* | | | |
| *Front* | *Other than front* | *Front* | | *Other than front* | |
| M1 | Ar4m | Ar4m | Ar4m | | Ar4m | | B, Br3, Br4m | - |
| M2 < 3.5 t | Ar4m, Ar4Nm | Ar4m, Ar4Nm | Ar4m, Ar4Nm | | Ar4m, Ar4Nm | | Br3, Br4m, Br4Nm | - |
| M2 > 3.5 t | Br3, Br4m, Br4Nm, or Ar4m or Ar4Nm ● | Br3, Br4m, Br4Nm, or Ar4m or Ar4Nm ● | Br3, Br4m, Br4Nm or Ar4m or Ar4Nm ● | | Br3, Br4m, Br4Nm or Ar4m or Ar4Nm ● | | Br3, Br4m, Br4Nm | - |
| M3 | See para. 8.1.7. for conditions when a lap belt is permitted | See para. 8.1.7. for conditions when a lap belt is permitted | See para. 8.1.7. for conditions when a lap belt is permitted | | See para. 8.1.7. for conditions when a lap belt is permitted | |  | B, Br3, Br4m, Br4Nm |
| N1 | Ar4m, Ar4Nm | Ar4m, Ar4Nm, Br4m, Br4Nm Ø | B, Br3, Br4m, Br4Nm or A, Ar4m, Ar4Nm\* 1 | | B, Br3, Br4m, Br4Nm | | B, Br3, Br4m, Br4Nm | - |
|  | Para. 8.1.2.1. lap belt permitted if seat is inboard of a passageway | Para. 8.1.6. lap belt permitted if the windscreen is not in the reference zone | |  | |  | - |
| N2  N3 | Br3, Br4m, Br4Nm orAr4m, Ar4Nm\* | **B, Br3, Br4m, Br4Nm** | B, Br3, Br4m, Br4Nm, or A, Ar4m, Ar4Nm\* | | **B, Br3, Br4m, Br4Nm** | | **B, Br3, Br4m, Br4Nm** | - |
| Para. 8.1.6. lap belt permitted if the windscreen is outside the reference zone and for the driver's seat | Para. 8.1.6. lap belt permitted if the windscreen is not in the reference zone | | - |
| A: three-point (lap and diagonal) belt | | B: 2-point (lap) belt | | r: retractor | | m: emergency locking retractor with multiple sensitivity | | |
| 3: automatically locking retractor | | 4: emergency locking retractor | | N: higher response threshold | | (see Regulation No. 16, paras. 2.14.3. and 2.14.5.) | | |
| \*: Refers to para. 8.1.6. of this Regulation 2 | | Ø: Refers to para. 8.1.2.1. of this Regulation | | ●: refers to para. 8.1.7. of this Regulation2 | |  | | |

1 Erratum to Supplement 12 to the 04 series of amendments, applicable "*ab initio*."

2 Erratum to Revision 4, applicable "*ab initio*."

*Note*: In all cases all S-type belts may be fitted in place of all possible A or B type belts, provided their anchorages comply with Regulation No. 14.

Where a harness belt has been approved as a S-type belt according to this Regulation, using the lap belt strap, the shoulder belt straps and possibly one or more retractors, one or two additional crotch straps including their attachments for their anchorages may be provided by the manufacturer/applicant. These additional anchorages need not meet the requirements of Regulation No. 14 (Erratum to Supplement 14 to the 04 series of amendments, applicable "*ab initio*.")."

II. Justification

1. In the current table of Annex 16 it may be difficult to determine if the outboard seating position (other than front) and centre seating position (other than front) are covered by the seatbelt requirement for vehicle category N3.

2. The proposal aims to avoid further misunderstandings. Thus it is suggested that a few other separations in the table are to be removed, due to the fact that the separations may lead to the possibility of misinterpretation of the table.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2014–2018 (ECE/TRANS/240, para. 105 and ECE/TRANS/2014/26, programme activity 02.4), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)