UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/737
31 August 2000

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

DRAFT SUPPLEMENT 1 TO THE 03 SERIES OF AMENDMENTS

TO REGULATION No. 24

(Visible pollutants)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its fifteenth session, following the recommendation by WP.29 at its one-hundred-and-twenty-first session. It is based on document TRANS/WP.29/2000/39, not amended (TRANS/WP.29/735, para. 114).

__________

GE.00-

Annex 8, paragraph 3.3., amend to read:

"3.3.	Light source

The light source shall be an incandescent lamp with a colour temperature in the range of 2800 to 3250 K or a green light-emitting diod (LED) with a spectral peak between 550 and 570 nm. The light source shall be protected against sooting by means that do not influence the optical path length beyond the manufacturer's specifications."

____________