UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/750
8 December 2000

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

CORRIGENDUM 4 TO THE 03 SERIES OF AMENDMENTS

TO REGULATION No. 44

(Child restraints)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its sixteenth session, following the recommendation by WP.29 at its one-hundred-and-twenty-second session. It is based on document TRANS/WP.29/2000/56, not amended (TRANS/WP.29/743, para. 153).

__________

GE.00-

Paragraph 11., correct to read:

"11.	CONFORMITY OF PRODUCTION

The conformity of production procedures shall comply with those set out in the Agreement, appendix 2 (E/ECE/324-E/ECE/TRANS/505/Rev.2), with the following requirements:

11.1.	Any child restraint system approved to this Regulation shall be so manufactured as to conform to the type approved by meeting the requirements set forth in paragraphs 6 to 8 above.

11.2.	The minimum requirements for conformity of production control procedures set forth in Annex 16 to this Regulation shall be complied with.

11.3.	The authority which has granted type approval may at any time verify the conformity control methods applied in each production facility. The normal frequency of these verifications shall be twice a year."

__________