|  |  |
| --- | --- |
|  | **INF.28** |
| **Economic Commission for Europe**Inland Transport Committee**Working Party on the Transport of Dangerous Goods****Joint Meeting of Experts on the Regulations annexed to theEuropean Agreement concerning the International Carriageof Dangerous Goods by Inland Waterways (ADN)(ADN Safety Committee)****Thirty-sixth session**Geneva, 27-31 January 2020Item 3 (c) of the provisional agenda**Implementation of the European Agreement concerning the International Carriage of Dangerous Goods by Inland Waterways (ADN):interpretation of the Regulations annexed to AND** |  29 January 2020German |

 Muster des Zulassungszeugnisses in ADN 8.6.1.3

 Übermittelt von EBU/ESO

 Ziffer 10 des Zulassungszeugnisses lautet:

10. Autonome Schutzsysteme

 ● Explosionsgruppe / Untergruppe der Explosionsgruppe II B: …..

Engl. ● Explosion group/subgroup of explosion group II B: ….....

EBU / ESO schlägt vor, die Worte “der Explosionsgruppe II B / of explosion group II B” zu streichen, so dass der betreffende Punkt lautet:

10. Autonome Schutzsysteme

 ● Explosionsgruppe / Untergruppe: ………

Engl. ● Explosion group/subgroup: ……..

Die vorgeschlagene Darstellung ist klarer. Im ADN wird ansonsten immer nur von Explosionsgruppe / Untergruppe gesprochen.