Proposal for supplement 1 to the 06 series of amendments to UN Regulation No. 110 (CNG and LNG vehicles)

Submitted by expert from the Netherlands [[1]](#footnote-2)\*

The text reproduced below was prepared by the Netherlands to amend UN Regulation No. 110. The modifications to the current text are marked in “bold black“ for new or strikethrough for deleted characters.

I. Proposal

*Annex 5R, paragraph 1.5.,* amend to read:

“1.5. Acceptable results

PRDs (temperature triggered) that have been tested according to the tests outlined in paragraph ~~3.1.2.~~**1.3.2.**, shall activate within two minutes of the recorded base line activation time of the samples listed in paragraph **1.**3.1.”

II. Justification

The above proposal is intended to correct references to paragraphs 1.3.2. instead of 3.1.2. and 1.3.1. instead of 3.1

1. \* In accordance with the programme of work of the Inland Transport Committee for 2024 as outlined in proposed programme budget for 2024 (A/78/6 (Sect. 20), table 20.5), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)